Labeling

 **VFD**

Equipment type abbreviated (variable frequency drive (VFD))

The piece of equipment it serves (ie hot water pump and whatever number it is, (HW#)

Panel or disconnect that power is coming from (EBP15-5)

Tag should read - - - VFD-HW#-EBP15-15

Translation - - - Variable Frequency Drive-Equipment Server-Panel-Circuit

**Starter**

Equipment type abbreviated (Starter (ST))

The piece of equipment it serves (ie hot water pump and whatever number it is, (HW#)

Panel or disconnect that power is coming from (EBP15-5)

Tag should read - - -  ST-HW#-EBP15-15

Translation - - - Starter–Equipment served–Panel-Circuit

**Disconnect**

Equipment type abbreviated (Disconnect (Dx))

The piece of equipment it serves (ie hot water pump and whatever number it is, ie (HW#)

Panel or disconnect that power is coming from ie (EBP15-5)

Tag should read - - -  Dx-HW#-EBP15-15

Translation - - - Disconnect – Equipment served – Panel - Circuit

**For the pumps :**

Hot Water Pump # (HW#)

Chilled Water Pump (CHW#)

Processed water pump (PW#)

Condenser Water (CW#)

Air Compressor – AC

Vacuum compressor – VC

Amalgum Seperator Skid - AMS

**For BAS -** Newly installed BAS cabinets, like with an AHU should read

BAS-AHU#-Circuit# (BAS-AHU8-EBP15-15)

